//1st program  write a program to light the led connector to pin number 13 will on for 4 second and off for 1 second

void setup() {

  // put your setup code here, to run once:

  pinMode(13,OUTPUT);

}

void loop() {

  // put your main code here, to run repeatedly:

  digitalWrite(13,HIGH);

  delay(4000);

  digitalWrite(13,low);

  delay(1500);

}